|  | TCP Applet
Transmisson Control Protocol (TCP)
Introduction Main window Menu Finite State Machine Application windows (Telnet / FTP) Channel | Start the Applet
Introduction
TCP/IP is made up of two acronyms, TCP, for Transmission Control Protocol, and IP, for Internet Protocol. TCP handles packet flow between systems and IP handles the routing of packets. However, that is a simplistic answer that we will expound on further. All modern networks are now designed using a layered approach. Each layer presents a predefined interface to the layer above it. By doing so, a modular design can be developed so as to minimize problems in the development of new applications or in adding new interfaces. The ISO/OSI protocol with seven layers is the usual reference model. Since TCP/IP was designed before the ISO model was developed it has five layers; however the differences between the two are mostly minor. 7. Application -- End user services such as email. 6. Presentation -- Data problems and data compression 5. Session -- Authenication and authorization 4. Transport -- Gaurentee end-to-end delivery of packets 3. Network -- Packet routing 2. Data Link -- Transmit and receive packets 1. Physical -- The cable or physical connection itself. |
TCP/IP-Reference Model
Application-Layer
Transport-Layer
Network-Layer
Datalink-Layer
Physical-Layer
Application Layer: Some of the applications we will cover are SMTP (mail), Telnet, FTP, Rlogin, NFS, NIS, and LPD Transport Layer: The transport uses two protocols, UDP and TCP. UDP which stands for User Datagram Protocol does not gaurentee packet delivery and applications which use this must provide their own means of verifying delivery. TCP does gaurentee delivery of packets to the applications which use it. |
Main Window
Menu
Menu "Options": "Userlevel" : contains two possible levels: "Beginner" and "Advanced". In the beginner mode, only TCP open- and close- connection can be investigated . In "Advanced" - Mode user can investigate the and simulate the following two applications (Telnet and FTP) "Graphics": In this menu, the user can choose between arrows and channel-pictures to present the data transfer between client and server. "Ouit": ends the applet execution. Menu "Screen": the size of the applet window can be changed according to the values choosen. Menü "Modus": only usable in the “Beginner” level. It turns the "Automaticmodus" on. |
Buttons
Start-button in the in the user level "Beginner": This button serves to cause an automatic opening of a connection.. The right Host first leads a passive Open and comes through it into the condition " LISTEN ". The left Host leads an active Open. Close-Button: This button appears after the successful connection-open operation to close it. Clear History Panel: Cause an erasure of the History. Reset: Causes a reset of the simulation. TCP FINITE STATE MACHINE: when activing this button, a new displaying the TCP-Finite State Machine will be launched. |
TCP Finite State Machine
The shaded drawn arrows in this finite state machine characterize a state change of the server the thickly drawn arrows characterize a a state change of a Client mark |
Applications (Telnet & FTP)
Buttons Servers: Cause a passive opening of a connection Dismiss: Close the window without finishing the execution of the application Abort: break the execution of the application up Client: Cause an active opening of a connection Ports Local Port of the application Dest. Port: destination port on the other machine Checkboxen TELNET: the Telnet protocol will be choosen as an application. It has two buttons: Push: all data will be transmitted immediately. Auto send: causes an automatic send of the data to be transmitted FTP: the FTP protocollwill be choosen | Telnet FTP
Channel
Choosing Error "ERROR" one can simulate a network error on the chanel. Two possible errors can be simulated: "Bit-Error" where the "Error-Rate" can be adjusted, and "Kill Segment" Choosing "Delay on" the datatransfer will be delated. In the textfield the delay in “milli second” (between 0 and 700) can be given, while choosing “Random” a delay value between 0 und 700 ms will be randomely generated. |

If you have any question, please do not hesitate to contact me @: Abdulmotaleb.El-Saddik@kom.tu-darmstadt.de