~Version Information
 VERS.                1.20:   CWLS LOG ASCII STANDARD -VERSION 1.20
 WRAP.                  NO:   One line per depth step         
~WELL INFORMATION BLOCK
#MNEM.UNIT       DATA TYPE    INFORMATION
#---------    -------------   ------------------------------
 STRT.F             91.00000 :
 STOP.F           3250.50000 :
 STEP.F              0.50000 :
 NULL.            -999.25000 : Null value 
 COMP.      COMPANY          : CITY OF ALBUQUERQUE                     
 WELL.      WELL             : CHARLES 5                               
 FLD .      FIELD            : CHARLES                                 
 LOC .      LOCATION         : NW 1/4, SW 1/4, SW 1/4                  
 LOC1.      LOCATION1        :                                         
 COUN.      COUNTY           : BERNALILLO                              
 STAT.      STATE            : NEW MEXICO                              
 NATI.      COUNTRY          :                                         
 DATE.      LOG DATE         : 19-JAN-1989                             
 API .      API NUMBER       : N/A                                     
 SECT.      SECTION          : 12                                      
 TOWN.      TOWNSHIP         : 10N                                     
 RANG.      RANGE            : 3E                                      
 DAY .      LOG DAY          : 19                                      
 MONT.      LOG MONTH        : 1                                       
 YEAR.      LOG YEAR         : 89                                      
 DMF .      DRILLING REF     : KB                                      
 LMF .      LOGGING  REF     : GL                                      
 PDAT.      PERMANENT DATUM  : GL                                      
 ENGI.      LOGGING ENGINEER : D.K. JUSTIS                             
 WITN.      LOGGING WITNESS  : RUSS CARLEN & R. NEWCOMER               
 LATI.      LATITUDE         :                                         
 LONG.      LONGITUDE        :                                         
 LUL .      LOGGING DISTRICT : FARMINGTON                              
 LUN .      LOGGING UNIT NO. : 8226                                    
 RUN .      LOGGING RUN NO.  : ONE                                     
 SON .      SERVICE ORDER NO.: 503998                                  
 SRVC.      SERVICE COMPANY  :   Schlumberger Well Services              
~CURVE INFORMATION
#MNEM.UNIT      API CODE      CURVE DESCRIPTION
#---------    -------------   ------------------------------
 DEPT.F     0      :  1  Depth
 DT  .US/F 6052080 :  2 DELTA-T                                 
 CGR .GAPI 3131001 :  3 Computed GR from Thor., Uran., Pota.    
 NPHI.     3189000 :  4 Neutron Porosity N                      
 POTA.     3171950 :  5 Potassium                               
 SGR .GAPI 3131001 :  6 Spectroscopy Gamma-Ray                  
 THOR.PPM  3179050 :  7 Thorium                                 
 URAN.PPM  3179250 :  8 Uranium                                 
 GR  .GAPI 7310010 :  9 Gamma Ray                               
 ILD .OHMM 7120460 : 10 Deep  Induction Standard Resistivity    
 ILM .OHMM 7120440 : 11 Medium Induction Standard Resistivity   
 SFLU.OHMM 7220010 : 12 SFL Resistivity (unaveraged)            
 SP  .MV   7010010 : 13 Spontaneous Potential                   
 CALI.IN   4528001 : 14 Caliper                                 
 DRHO.G/C3 4535601 : 15 Delta  RHO                              
 PEF .     4535801 : 16 Photoelectric Factor                    
 RHOB.G/C3 4535002 : 17 Bulk Density                            
~PARAMETER INFORMATION
#MNEM.UNIT        VALUE       DESCRIPTION
#---------    -------------   ------------------------------
 BHT .DEGF N/A              : Bottom Hole Temperature                 
 BS  .IN   9.875            : Bit Size                                
 MDEN.G/C3 N/A              : Matrix Density                          
 DFD .LB/G 9.4              : Drilling Fluid Density                  
 DFV .S    42.              : Drilling Fluid Viscosity                
 DFL .C3   11.              : Drilling Fluid Loss                     
 RMFS.OHMM 8.625            : Resistivity of Mud Filtrate Sample      
 EKB .F    5229.            : Elevation of Kelly Bushing              
 EGL .F    5219.            : Elevation of Ground Level               
 BLI .F    3237.            : Bottom Log Interval                     
 BSAL.PPM  0.               : Borehole Salinity                       
 FLEV.F    -50000.          : Fluid Level                             
 MCST.DEGF 68.              : Mud Cake Sample Temperature             
 MFST.DEGF 68.              : Mud Filtrate Sample Temperature         
 MRT .DEGF 89.              : Maximum Recorded Temperature            
 MST .DEGF 68.              : Mud Sample Temperature                  
 RMCS.OHMM 20.13            : Resistivity of Mud Cake Sample          
 RMS .OHMM 11.5             : Resistivity of Mud Sample               
 RW  .OHMM 1.               : Resistivity of Water                    
 TDD .F    3240.            : Total Depth - Driller                   
 TDL .F    3243.            : Total Depth - Logger                    
 TLI .F    104.             : Top Log Interval                        
~OTHER INFORMATION
#MNEM.UNIT    VALUE                                 DESCRIPTION
#---------    -----------------------------------   ----------------------------
 HIDE.     COMPENSATED NEUTRON LOG                 : Header Identifer           
 MATR.     N/A                                     : Matrix                     
 FNUM.     1.                                      : F-Numerator for Formation F
 FEXP.     2.                                      : F-Exponent for Formation Fa
 DFT .     LOW-GEL                                 : Drilling Fluid Type        
 DFPH.     7.                                      : Drilling Fluid Ph          
 MCSS.     CALCULATED                              : Mud Cake Sample Source     
 MFSS.     CALCULATED                              : Mud Filtrate Sample Source 
 FD  .     N/A                                     : Fluid Density              
 MSS .     MUD TANK                                : Mud Sample Source          
 OS1 .     FDC/AMS                                 : Other Services Line 1      
 OS2 .     DIL                                     : Other Services Line 2      
 OS3 .     CNT/NGT                                 : Other Services Line 3      
 OS4 .     BHC                                     : Other Services Line 4      
 OS5 .     CST                                     : Other Services Line 5      
 OS6 .                                             : Other Services Line 6      
 R1  .     TOOL STRING:  CNTH NGTD TCCB            : Remark Line 1              
 R2  .                                             : Remark Line 2              
 R3  .                                             : Remark Line 3              
 R4  .                                             : Remark Line 4              
 R5  .                                             : Remark Line 5              
 R6  .                                             : Remark line 6              
 R7  .                                             : Remark line 7              
 R8  .     CREW:  SANDERS & RUGO                   : Remark line 8              
 HIDE.     DUAL INDUCTION                          : Header Identifer           
 MATR.     1.0                                     : Neutron Matrix (1=SAND)    
 FNUM.     1.                                      : F-Numerator for Formation F
 FEXP.     2.                                      : F-Exponent for Formation Fa
 DFT .     LOW-GEL                                 : Drilling Fluid Type        
 DFPH.     7.                                      : Drilling Fluid Ph          
 MCSS.     CALCULATED                              : Mud Cake Sample Source     
 MFSS.     CALCULATED                              : Mud Filtrate Sample Source 
 FD  .     N/A                                     : Fluid Density              
 MSS .     MUD TANK                                : Mud Sample Source          
 OS1 .     FDC/AMS                                 : Other Services Line 1      
 OS2 .     DIL                                     : Other Services Line 2      
 OS3 .     CNT/NGT                                 : Other Services Line 3      
 OS4 .     BHC                                     : Other Services Line 4      
 OS5 .     CST                                     : Other Services Line 5      
 OS6 .                                             : Other Services Line 6      
 R1  .     TOOL STRING:  DITD SGTE                 : Remark Line 1              
 R2  .     1.5 INCH STANDOFF USED ON THE INDUCTION.: Remark Line 2              
 R3  .                                             : Remark Line 3              
 R4  .                                             : Remark Line 4              
 R5  .                                             : Remark Line 5              
 R6  .                                             : Remark line 6              
 R7  .                                             : Remark line 7              
 R8  .     CREW:  SANDERS & RUGO                   : Remark line 8              
 HIDE.     DUAL INDUCTION                          : Header Identifer           
 MATR.     N/A                                     : Matrix                     
 FNUM.     N/A                                     : F-Numerator for Formation F
 FEXP.     N/A                                     : F-Exponent for Formation Fa
 DFT .     LOW-GEL                                 : Drilling Fluid Type        
 DFPH.     7.                                      : Drilling Fluid Ph          
 MCSS.     CALCULATED                              : Mud Cake Sample Source     
 MFSS.     CALCULATED                              : Mud Filtrate Sample Source 
 FD  .     N/A                                     : Fluid Density              
 MSS .     MUD TANK                                : Mud Sample Source          
 OS1 .     FDC/AMS                                 : Other Services Line 1      
 OS2 .     DIL                                     : Other Services Line 2      
 OS3 .     CNT/NGT                                 : Other Services Line 3      
 OS4 .     BHC                                     : Other Services Line 4      
 OS5 .     CST                                     : Other Services Line 5      
 OS6 .                                             : Other Services Line 6      
 R1  .     TOOL STRING:  DITD SGTE                 : Remark Line 1              
 R2  .     1.5 INCH STANDOFF USED ON THE INDUCTION.: Remark Line 2              
 R3  .                                             : Remark Line 3              
 R4  .                                             : Remark Line 4              
 R5  .                                             : Remark Line 5              
 R6  .                                             : Remark line 6              
 R7  .                                             : Remark line 7              
 R8  .     CREW:  SANDERS & RUGO                   : Remark line 8              
 HIDE.     TEMPERATURE LOG                         : Header Identifer           
 MATR.     N/A                                     : Matrix                     
 FNUM.     1.                                      : F-Numerator for Formation F
 FEXP.     2.                                      : F-Exponent for Formation Fa
 DFT .     LOW-GEL                                 : Drilling Fluid Type        
 DFPH.     7.                                      : Drilling Fluid Ph          
 MCSS.     CALCULATED                              : Mud Cake Sample Source     
 MFSS.     CALCULATED                              : Mud Filtrate Sample Source 
 FD  .G/C3 0.9999999                               : Fluid Density              
 MSS .     MUD TANK                                : Mud Sample Source          
 OS1 .     FDC/AMS                                 : Other Services Line 1      
 OS2 .     DIL                                     : Other Services Line 2      
 OS3 .     CNT/NGT                                 : Other Services Line 3      
 OS4 .     BHC                                     : Other Services Line 4      
 OS5 .     CST                                     : Other Services Line 5      
 OS6 .                                             : Other Services Line 6      
 R1  .     TOOL STRING:  LDTC SGTL TCCB AMS        : Remark Line 1              
 R2  .     LOGGED ON A SANDSTONE MATRIX = 2.65     : Remark Line 2              
 R3  .     TEMPERATURE LOGGED DOWN.                : Remark Line 3              
 R4  .                                             : Remark Line 4              
 R5  .                                             : Remark Line 5              
 R6  .                                             : Remark line 6              
 R7  .                                             : Remark line 7              
 R8  .     CREW:  SANDERS & RUGO                   : Remark line 8              
~A       