Independent Sinusoidal Voltage Source
Model Name | SINE(V1)
Symbol |
Generics |
Name | Type | Default | Unit | Min | Description
V0 | REAL | 0.0 | V |  | offset voltage
A | REAL | 1.0 | V |  | amplitude
FREQ | REAL | 50.0 | Hz | 0.0 | frequency
Ports |
Interface | Name | Type/Nature | Description
terminal | P | ELECTRICAL | positive terminal
terminal | N | ELECTRICAL | negative terminal
Description | P and N are the positive and negative terminals, respectively. The value of the voltage source is equal to V0+A*SIN(2*pi*FREQ*t).
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench