<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/bench.png</symbol>
  <comments>
    <title>Test-bench for Sample and Hold Block</title>
    <model_name>BENCH(BENCH_SAMPLE_AND_HOLD)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>A 1 kHz sinusoidal voltage is sampled after 250 us with a period<br></br>of 50 us. The simulation should run until 1 ms. <br></br><br></br></description>
    <link_source><A HREF="../src/bench.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>SAMPLE_AND_HOLD(IDEAL)</design_unit>
    </dependency>
  </comments>
  <interface>
  </interface>
</model>
