<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/p_sin.png</symbol>
  <comments>
    <title>Sinusoidal source with power specification</title>
    <model_name>P_SIN(SINGLE_TONE)<br></br>P_SIN(TWO_TONE)<br></br>P_SIN(AM)<br></br>P_SIN(SFFM)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>The model describes independent and modulated sources<br></br>where the amplitude is specified in terms of power.<br></br>There are architectures with single- and two-tone<br></br>as well as amplitude and frequency modulted sine waves<br></br>available.<br></br></description>
    <link_source><A HREF="../src/p_sin.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>IEEE</library>
      <design_unit>MATH_REAL</design_unit>
    </dependency>
  </comments>
  <interface>
    <parameter>
      <name>VO</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>V</unit>
      <comment> offset voltage </comment>
    </parameter>
    <parameter>
      <name>PA_DBM</name>
      <type>REAL</type>
      <default>-100.0</default>
      <unit>dBm</unit>
      <comment> first tone amplitude </comment>
    </parameter>
    <parameter>
      <name>FREQ</name>
      <type>REAL</type>
      <default>1.0e03</default>
      <unit>Hz</unit>
      <comment> first tone frequency </comment>
    </parameter>
    <parameter>
      <name>PHASE</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>rad</unit>
      <comment> first tone phase </comment>
    </parameter>
    <parameter>
      <name>PA2_DBM</name>
      <type>REAL</type>
      <default>-100.0</default>
      <unit>dBm</unit>
      <comment> second tone amplitude </comment>
    </parameter>
    <parameter>
      <name>FREQ2</name>
      <type>REAL</type>
      <default>1.0e03</default>
      <unit>Hz</unit>
      <comment> second tone frequency </comment>
    </parameter>
    <parameter>
      <name>PHASE2</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>rad</unit>
      <comment> second tone phase </comment>
    </parameter>
    <parameter>
      <name>FREQM</name>
      <type>REAL</type>
      <default>1.0</default>
      <unit>Hz</unit>
      <comment> modulating tone frequency </comment>
    </parameter>
    <parameter>
      <name>PHASEM</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>rad</unit>
      <comment> modulating tone phase </comment>
    </parameter>
    <parameter>
      <name>MDI</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>-</unit>
      <comment> modulation index </comment>
    </parameter>
    <parameter>
      <name>ROUT</name>
      <type>REAL</type>
      <default>50.0</default>
      <unit>Ohm</unit>
      <comment> output impedance </comment>
    </parameter>
    <port>
      <port_id>terminal</port_id>
      <name>P</name>
      <port_type>ELECTRICAL</port_type>
      <comment> positive terminal</comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>M</name>
      <port_type>ELECTRICAL</port_type>
      <comment> negative terminal</comment>
    </port>
  </interface>
</model>
