<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/bench.png</symbol>
  <comments>
    <title>Test-bench for Lossless Line</title>
    <model_name>BENCH(BENCH_LOSSLESS_LINE)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>The voltage pulse at node N1 is delayed by 1.5 ms.<br></br>An ideal transmission is carried out if the load<br></br>resistor equals the characteristic impedance of the<br></br>lossless line. The default value of the characteristic<br></br>impedance is 50 Ohm. The simulation should run until 10 ms. <br></br>Simulation parameters (hmax, eps) should be carefully<br></br>chosen.<br></br><br></br></description>
    <link_source><A HREF="../src/bench.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>V_SOURCE(IDEAL)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>LINE(LOSSLESS)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>RESISTOR(V1)</design_unit>
    </dependency>
  </comments>
  <interface>
  </interface>
</model>
