WLAN receiver
Model Name | RECEIVER(DOUBLE_CONV)
Symbol |
Ports |
Interface | Name | Type/Nature | Description
terminal | P_RF | ELECTRICAL |
terminal | P_CTRL | ELECTRICAL |
terminal | P_GND | ELECTRICAL |
terminal | P_I | ELECTRICAL |
terminal | P_Q | ELECTRICAL |
terminal | P_VDD | ELECTRICAL |
Description | This model describes the complete RF front end of a WLAN receiver according to IEEE802.11a standard. The receiver has a double conversion architecture where the same local oscillator frequency is applied twice in order to mix the signal from passband down to baseband.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
WORK | VCO(ANALOG)
WORK | LNA(RF)
WORK | MIXER(RF)
WORK | LOWPASS(BHV_RF)
WORK | PLL(LINEAR)
WORK | SPLITTER(IDEAL)
WORK | SHIFTER(IDEAL)
Source | See source code
Example | See test-bench