Sinusoidal source with power specification
Model Name | P_SIN(SINGLE_TONE) P_SIN(TWO_TONE) P_SIN(AM) P_SIN(SFFM)
Symbol |
Generics |
Name | Type | Default | Unit | Description
VO | REAL | 0.0 | V | offset voltage
PA_DBM | REAL | -100.0 | dBm | first tone amplitude
FREQ | REAL | 1.0e03 | Hz | first tone frequency
PHASE | REAL | 0.0 | rad | first tone phase
PA2_DBM | REAL | -100.0 | dBm | second tone amplitude
FREQ2 | REAL | 1.0e03 | Hz | second tone frequency
PHASE2 | REAL | 0.0 | rad | second tone phase
FREQM | REAL | 1.0 | Hz | modulating tone frequency
PHASEM | REAL | 0.0 | rad | modulating tone phase
MDI | REAL | 0.0 | - | modulation index
ROUT | REAL | 50.0 | Ohm | output impedance
Ports |
Interface | Name | Type/Nature | Description
terminal | P | ELECTRICAL | positive terminal
terminal | M | ELECTRICAL | negative terminal
Description | The model describes independent and modulated sources where the amplitude is specified in terms of power. There are architectures with single- and two-tone as well as amplitude and frequency modulted sine waves available.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code