Digital-to-analog converter
Model Name | D2A(BHV_RF)
Symbol |
Generics |
Name | Type | Default | Unit | Min | Description
PMAX_DBM | REAL | -100.0 | dBm |  | maximum power amplitude
TRISE | REAL | 1.0E-9 | s |  | transition time for rising edge
TFALL | REAL | 1.0E-9 | s |  | transition teim for falling edge
ROUT | REAL | 50.0 | Ohm | >0.0 | output resistance
Ports |
Interface | Name | Type/Nature | Mode | Description
terminal | A | ELECTRICAL |  | analog output
terminal | GND | ELECTRICAL |  | analog ground
signal | D | BIT_VECTOR | in | digital input
Description | This model describes a digital to analog converter. The conversion is done in a digital process at every change of the digital input signal. The transition to the analog domain includes a 'RAMP attribute where the transistion times can be parameterized.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code
Example | See test-bench