Linear Voltage-Controlled Voltage Source with RI and ROUT
Model Name | VCVS_R(V1)
Symbol |
Generics |
Name | Type | Default | Unit | Description
V | REAL | 1.0 |  | voltage gain
RIN | REAL | 50.0 | Ohm | input resistor
ROUT | REAL | 50.0 | Ohm | output resistor
Ports |
Interface | Name | Type/Nature | Description
terminal | IN1 | ELECTRICAL | controlling plus terminal
terminal | IN2 | ELECTRICAL | controlling minus terminal
terminal | OUTP | ELECTRICAL | output plus terminal
Description | IN1 and IN2 are the positive and negative controlling terminals, respectively. The input voltage controls the output voltage. V is the voltage gain. RI is the input resistor between IN1 and IN2. ROUT is the outout resitor.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench