Wobble generator
Model Name | WOBBLE(BHV)
Symbol |
Generics |
Name | Type | Default | Unit | Description
INITDELAY | REAL | 0.0 | s | initial time delay before oscillation starts
STARTFREQ | REAL | 1.0 | Hz | initial frequency where sweep starts
SWEEPRATE | REAL | 1.0 | Hz/s | rate of change for frequency sweep
STOPFREQ | REAL | 1.0e7 | Hz | end frequency where sweep stops
AMP_DBM | REAL | -100.0 | dBm | power amplitude of sine wave
ROUT | REAL | 50.0 | Ohm | output resistance
Ports |
Interface | Name | Type/Nature | Description
terminal | P | ELECTRICAL | positive terminal
terminal | M | ELECTRICAL | negative terminal
Description | The model describes a sine wave where the frequency sweeps over a given range from STARTFREQ to STOPFREQ. The amplitude of the sine wave is given in term sof power.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code