Analog Voltage Controlled Oscillator
Model Name | VCO(BASIC)
Symbol |
Generics |
Name | Type | Default | Unit | Description
F0 | REAL | 1.0 | Hz | center frequency
KF | REAL | 1.0 | Hz/V | gain
AMPL | REAL | 1.0 | V | amplitude
PHI0 | REAL | 0.0 | rad | initial phase
Ports |
Interface | Name | Type/Nature | Description
terminal | INP | ELECTRICAL | input terminal
terminal | OUTP | ELECTRICAL | output terminal
Description | The model describes a VCO. The frequency of the output voltage source is controlled by the input voltage. The frequency equals KF*VIN + F0.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code
Example | See test-bench