Piece-Wise Linear Quantity Source
Model Name | QPWL(BASIC)
Symbol |
Generics |
Name | Type | Default | Unit | Description
WAVE | REAL_VECTOR |  |  | time value pairs T1/ V1/ T2/ V2/ ...
Ports |
Interface | Name | Type/Nature | Mode | Description
quantity | OUTP | REAL | out | output
Description | The model describes a PWL nonconservative source in a similar way as a SPICE piece-wise independent voltage source. The parameter WAVE is a one dimensional real array with time value pairs T1, V1, T2, V2, ... Each pair of values Ti, Vi specifies that the value of the source is Vi at time Ti. The value of the source at intermediate values is determined by using linear interpolation. The times must be given in ascending order.
References | T. Quarles et al: SPICE3 Version 3f3 User's Manual. University of California, May 1993. Model Library FUNDAMENTALS_VDA of VDA/FAT-AK30: http://fat-ak30.eas.iis.fraunhofer.de
Source | See source code
Example | See test-bench