<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/bench.png</symbol>
  <comments>
    <title>Testbench for Voltage Sources</title>
    <model_name>BENCH(BENCH_SOURCES)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>The value of a sinusoidal voltage at N_SINE is gained by a voltage<br></br>controlled voltage source. This value at node N1times2 is gained<br></br>by a voltage controlled voltage source that considers input<br></br>and output resistors. The output node N_OUT is connected with<br></br>the electrical reference node by a resistor of 50 Ohm. The<br></br>simulation should run until 40 ms.<br></br><br></br></description>
    <link_source><A HREF="../src/bench.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>SINE(V1)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>VCVS(V1)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>VCVS_R(V1)</design_unit>
    </dependency>
  </comments>
  <interface>
  </interface>
</model>
