Test-bench for Lowpass Filter in AC Domain
Model Name | BENCH(BENCH_AC)
Description | The frequency characteristics of an analog and digital Bessel lowpass are determined. An AC analysis should be carried out between 10 Hz and 50 kHz (500 points/decade).
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
WORK | LOWPASS(BESSEL_2)
WORK | LOWPASS(BESSEL_2_DIGITAL)
Source | See source code
Results | See results