Test-bench for Lossless Line
Model Name | BENCH(BENCH_LOSSLESS_LINE)
Description | The voltage pulse at node N1 is delayed by 1.5 ms. An ideal transmission is carried out if the load resistor equals the characteristic impedance of the lossless line. The default value of the characteristic impedance is 50 Ohm. The simulation should run until 10 ms. Simulation parameters (hmax, eps) should be carefully chosen.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
WORK | V_SOURCE(IDEAL)
WORK | LINE(LOSSLESS)
WORK | RESISTOR(V1)
Source | See source code
Results | See results