Testbench for Voltage Sources
Model Name | BENCH(BENCH_SOURCES)
Description | The value of a sinusoidal voltage at N_SINE is gained by a voltage controlled voltage source. This value at node N1times2 is gained by a voltage controlled voltage source that considers input and output resistors. The output node N_OUT is connected with the electrical reference node by a resistor of 50 Ohm. The simulation should run until 40 ms.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
WORK | SINE(V1)
WORK | VCVS(V1)
WORK | VCVS_R(V1)
Source | See source code
Results | See results