Power measurement unit
Model Name | POWER_METER(FEEDTHROUGH) POWER_METER(TERMINATING)
Symbol |
Generics |
Name | Type | Default | Unit | Description
T_INTEG | real | 1.0e-03 | s | integration period
R_TERM | real | 50.0 | Ohm | termination resistance
Ports |
Interface | Name | Type/Nature | Mode | Description
terminal | P_1 | ELECTRICAL |  | first measurement pin
terminal | P_2 | ELECTRICAL |  | second measurement pin
quantity | P_DBM | REAL | out | output power
Description | This model describes a power measurement unit with two different architectures. The architecture feedthrough has no load resistance but measures the current flowing though it. The architecture terminating includes a termination resistor to match the resistance of the preceding block. The power is measured over an integration period of T_INTEG which is a model parameter and can therefore be adjusted.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code
Example | See test-bench