<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/bench.png</symbol>
  <comments>
    <title>Test-bench for A-to-D Converter</title>
    <model_name>BENCH(BENCH_A2D)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>A 1 kHz sinusoidal voltage is converted. Signal S_OUT_IDEAL is<br></br>equal '1' for voltages greater than 0.0 and '0' for voltages<br></br>less than 0.0. Signal S_OUT_EXTENDED is set to '1' when the<br></br>voltage crosses 0.25. It is set to '0' when the voltage is less<br></br>than -0.25. Simulation should run until 3 ms.<br></br><br></br></description>
    <link_source><A HREF="../src/bench.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>IEEE</library>
      <design_unit>STD_LOGIC_1164</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>A2D(IDEAL)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>A2D(EXTENDED)</design_unit>
    </dependency>
  </comments>
  <interface>
  </interface>
</model>
