<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/sample_and_hold.png</symbol>
  <comments>
    <title>Sample and Hold Block</title>
    <model_name>SAMPLE_AND_HOLD(IDEAL)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>The input voltage is sampled after time DELAY. The model<br></br>realizes a zero order sample and hold.<br></br><br></br></description>
    <link_source><A HREF="../src/sample_and_hold.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
  </comments>
  <interface>
    <parameter>
      <name>TSAMPLE</name>
      <type>REAL</type>
      <default>1.0E-3</default>
      <unit>s</unit>
      <min> &gt;0.0</min>
      <comment> sampling time </comment>
    </parameter>
    <parameter>
      <name>DELAY</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>s</unit>
      <min> 0.0 </min>
      <comment> delay </comment>
    </parameter>
    <port>
      <port_id>terminal</port_id>
      <name>INP</name>
      <port_type>ELECTRICAL</port_type>
      <comment> controlling terminal</comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>OUTP</name>
      <port_type>ELECTRICAL</port_type>
      <comment> output terminal</comment>
    </port>
  </interface>
</model>
