EScope5: Multiple waveforms
Escope5 takes advantage of the code refactoring carried out in the previous EScope versions to add a new feature with minimal changes in the codeplotting more than one waveform in the panel.

To add more than one waveform to the current panel it is necessary to select more than one node in the tree on the left panel. This is achieved "a la Windows" by holding the <ctrl> key when selecting tree nodes. Alternatively, a whole range of node can be defined by holding the <Shift key> when selecting tree nodes.

This application defines three panels. At the left side, when a database is open, the hierarchical structure is displayed and it is possible to navigate in the tree. The central panel dispplayes the current waveform(s). The top panel displays the current (X, Y) pair when the crosshair display option is defined.

The File Menu Bar option allows to:

- connect to a MDSplus server. The default server and port is localhost and 8000, i.e. a MDSplus data server running locally on port 8000 (the default configuration)
- open an experiment and shot. The default experiment and port is edam and 17615, respectively. They correspond to a database which is provided by the installer.
- exit from the application

The Graph Menu Bar option activates a pop-up panel which allows to

- associte a separate color to the graph title, the background and the plot line.
- define whether a border is defined arould the signal plot
- define which algorithm to use for computing tick numbers.
- define the current waveform interaction :
  - drag a crosshair over the waveform,
  - zoom a portion of the waveform by dragging the mouse to define a rectangle of interest. When the mouse is released, the enlarged portion of the waveform is displayed
  - grab the entire waveform.
  A double click restores the default confition, i.e. the whole waveform matted into the display window.
  The changes are applied when either Ok or Apply button is pressed.

To exercise this program the following steps are required:

1. If not already running, start a MDSplus data server. On windows, click on start->programs->MDSplus->MDSDataserver. On Linux, run script start_mdsip.
2. Change directory in <source root>/escopes/escope5, where <source root> is the directory where you copied the source directory in the CD.
3. Include the current directory in your CLASSPATH environmante variable. On Windows this can be done by changing the CLASSPATH definition in Control Panel/System setting, or by the command
   set CLASSPATH=.;%CLASSPATH%
   On Linux (bash shell) this can be done by the command
   export CLASSPATH=.:$CLASSPATH
4. Compile the java source files with the command
   javac *.java
5. Run the program with no arguments.
   java EScope5

When the edam database is open, valid signals are listed in the SIGNALS.PB subtree.

View Source