Independent Voltage Pulse Source
Model Name | V_SOURCE(PULSE)
Symbol |
Generics |
Name | Type | Default | Unit | Min | Description
AMPL | REAL | 1.0 | V |  | pulsed value
T_DELAY | TIME | 0.5ms | TIME |  | delay time
DURATION | TIME | 1ms |  |  |
T_RISE | REAL | 0.0 | s | >=0.0 | rise and fall time
Ports |
Interface | Name | Type/Nature | Description
terminal | P | ELECTRICAL | positive terminal
terminal | N | ELECTRICAL | negative terminal
Description | The model describes a voltage pulse source. The initial voltage is 0.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench