Phase shifter
Model Name | SHIFTER(IDEAL)
Symbol |
Generics |
Name | Type | Default | Unit | Description
RIN | REAL | 50.0 |  |
ROUT | REAL | 50.0 |  |
FREQ | REAL | 1.0 |  |
Ports |
Interface | Name | Type/Nature | Description
terminal | INP | ELECTRICAL | input
terminal | OUT0 | ELECTRICAL | 0 delay (cos)
terminal | OUT90 | ELECTRICAL |
Description | This model describes an ideal PI/4 phase shifter. The frequency of the input signal has to be provided as a parameter to the model.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench