<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/transmit.png</symbol>
  <comments>
    <title>Transmitter</title>
    <model_name>TRANSMIT(SIMPLE)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>This model describes the RF front end of a transmitter to be<br></br>used with the WLAN receiver model. Only one signal path is<br></br>implemented.<br></br></description>
    <link_source><A HREF="../src/transmit.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>IEEE</library>
      <design_unit>MATH_REAL</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>VCO(ANALOG)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>MIXER(RF)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>LOWPASS(BHV_RF)</design_unit>
    </dependency>
  </comments>
  <interface>
    <port>
      <port_id>terminal</port_id>
      <name>P_RF</name>
      <port_type>ELECTRICAL</port_type>
      <comment></comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>P_CTRL</name>
      <port_type>ELECTRICAL</port_type>
      <comment></comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>P_GND</name>
      <port_type>ELECTRICAL</port_type>
      <comment></comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>P_I</name>
      <port_type>ELECTRICAL</port_type>
      <comment></comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>P_Q</name>
      <port_type>ELECTRICAL</port_type>
      <comment></comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>P_VDD</name>
      <port_type>ELECTRICAL</port_type>
      <comment></comment>
    </port>
  </interface>
</model>
