Mixer
Model Name | MIXER(RF)
Symbol |
Generics |
Name | Type | Default | Unit | Min | Description
GP_DB | REAL | 0.0 | dB |  | power gain of stage
IP3_DBM | REAL | -20.0 | dBm |  | input referenced IP3
FNOISE_DB | REAL | 0.0 | dB |  | noise figure
RIN | REAL | 50.0 | Ohm | >0.0 | input resistance
RIN_CLK | REAL | 50.0 | Ohm | >0.0 | input resistance at clock input
ROUT | REAL | 50.0 | Ohm | >0.0 | output resistance
FG | REAL | REAL'HIGH | Hz | >0.0 | dominant pole
Ports |
Interface | Name | Type/Nature | Description
terminal | P_IN | ELECTRICAL | input pin
terminal | P_OUT | ELECTRICAL | output pin
terminal | P_CLOCK | ELECTRICAL | local oscillator pin
terminal | VDD | ELECTRICAL | supply voltage
terminal | GND | ELECTRICAL | reference terminal
Description | This model describes an analog mixer and includes the multiplier stage and amplifier properties like gain, compression and transfer function. Resistances at the input and output terminals are modeled as well.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code
Example | See test-bench