<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/bench.png</symbol>
  <comments>
    <title>Charge pump test bench</title>
    <model_name>BENCH(TEST_DPLL)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>The test-bench shows how a digital PLL is built up from<br></br>a phase-frequency detector, a charge pump, an integrator<br></br>and a VCO.<br></br></description>
    <link_source><A HREF="../src/bench.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
    <dependency>
      <library>IEEE</library>
      <design_unit>MATH_REAL</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>VCO(ANALOG)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>CP(SIMPLE)</design_unit>
    </dependency>
    <dependency>
      <library>WORK</library>
      <design_unit>PFD(A1)</design_unit>
    </dependency>
  </comments>
  <interface>
  </interface>
</model>
