Charge pump
Model Name | CP(SIMPLE)
Symbol |
Generics |
Name | Type | Default | Unit | Description
R_ISRC | REAL | 1.0e3 | Ohm | current sources resistance
ROUT | REAL | 50.0 | Ohm | output resistance
Ports |
Interface | Name | Type/Nature | Mode | Description
terminal | P_OUT | ELECTRICAL |  | output pin
terminal | VDD | ELECTRICAL |  | positive voltage
terminal | VSS | ELECTRICAL |  | negative voltage
signal | S_UP | BIT | IN | up signal
signal | S_DOWN | BIT | IN | down signal
Description | This models describes a simple charge pump which contains switchable resistances driven by a current source.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench