Linear Voltage-Controlled Voltage Source
Model Name | VCVS(V1)
Symbol |
Generics |
Name | Type | Default | Unit | Description
V | REAL | 1.0 |  | voltage gain
Ports |
Interface | Name | Type/Nature | Description
terminal | IN1 | ELECTRICAL | controlling plus terminal
terminal | IN2 | ELECTRICAL | controlling minus terminal
terminal | OUTP | ELECTRICAL | output plus terminal
Description | IN1 and IN2 are the positive and negative controlling terminals, respectively. The input voltage controls the output voltage between terminal OUTP end the electrical reference node. V is the voltage gain.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench