Phasedetector
Model Name | PD(BASIC)
Symbol |
Generics |
Name | Type | Default | Unit | Description
GAIN | REAL | 1.0 |  | gain
Ports |
Interface | Name | Type/Nature | Description
terminal | IN1 | ELECTRICAL | first input
terminal | IN2 | ELECTRICAL | second input
terminal | OUTP | ELECTRICAL | output terminal
Description | The model describes a mulitplier. The output voltage source equals the product of input voltages times GAIN. The model can be used as a phasedetector in an analog PLL description.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench