<?xml version="1.0" encoding="ISO-8859-1"?>
<?xml-stylesheet href="/usr/local/vamdoc-1.0.2-kluwer/config/model.xsl" type="text/xsl"?>
<!DOCTYPE model SYSTEM "/usr/local/vamdoc-1.0.2-kluwer/config/model.dtd"><model>
  <symbol>../symbol/integrator.png</symbol>
  <comments>
    <title>Integrator Block</title>
    <model_name>INTEGRAL_BLOCK(IDEAL)</model_name>
    <library>N/A</library>
    <structure>N/A</structure>
    <description>The ouput voltage is the integral of the input voltage. The<br></br>model is realized by a voltage-controlled voltage source.<br></br><br></br></description>
    <link_source><A HREF="../src/integrator.vhd">See source code</A></link_source>
    <dependency>
      <library>IEEE_proposed</library>
      <design_unit>ELECTRICAL_SYSTEMS</design_unit>
    </dependency>
  </comments>
  <interface>
    <parameter>
      <name>GAIN</name>
      <type>REAL</type>
      <default>1.0</default>
      <unit></unit>
      <comment> gain </comment>
    </parameter>
    <parameter>
      <name>IC</name>
      <type>REAL</type>
      <default>0.0</default>
      <unit>V</unit>
      <comment> initial value </comment>
    </parameter>
    <port>
      <port_id>terminal</port_id>
      <name>INP</name>
      <port_type>ELECTRICAL</port_type>
      <comment> controlling terminal</comment>
    </port>
    <port>
      <port_id>terminal</port_id>
      <name>OUTP</name>
      <port_type>ELECTRICAL</port_type>
      <comment> output terminal</comment>
    </port>
  </interface>
</model>
