First Order Lowpass and Pole-Zero Filter
Model Name | FILTER(LP) FILTER(PZ)
Symbol |
Generics |
Name | Type | Default | Unit | Description
GAIN | REAL | 1.0 |  | gain
FC | REAL | 1.0 | Hz | cut-off frequency
ZF | REAL | 1.0 | Hz | zero frequency
Ports |
Interface | Name | Type/Nature | Description
terminal | INP | ELECTRICAL | input terminal
terminal | OUTP | ELECTRICAL | output terminal
Description | The model describes an analog filter. The architecture LP realizes a first order lowpass filter with cut-off frequency FC. The architecture PZ realizes a pole-zero filter with pole frequency FC and zero frequency ZF.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
IEEE | MATH_REAL
Source | See source code
Example | See test-bench