Simple RC Subircuit
Model Name | RC(V1)
Symbol |
Generics |
Name | Type | Default | Unit | Min | Description
RES | REAL | 1.0 | Ohm | >0.0 | value of the resistor
CAP | REAL | 1.0 | F | >0.0 | value of the capacitor
Ports |
Interface | Name | Type/Nature | Description
terminal | T1 | ELECTRICAL | connected to resistor
terminal | T2 | ELECTRICAL | common node of resistor and capacitor
terminal | T3 | ELECTRICAL | connected to capacitor
Description | This example demonstrates how to create hierachical models. The terminals T1 and T2 are connected by a resistor. The terminals T2 and T3 are connected by a capacitor. It is required that the element values are positive.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
WORK | RESISTOR(V1)
WORK | CAPACITOR(V1)
Source | See source code
Example | See test-bench