Splitter
Model Name | SPLITTER(IDEAL)
Symbol |
Generics |
Name | Type | Default | Unit | Description
RIN | REAL | 50.0 |  |
ROUT | REAL | 50.0 |  |
Ports |
Interface | Name | Type/Nature | Description
terminal | P_I | ELECTRICAL |
terminal | GND | ELECTRICAL |
terminal | P_O1 | ELECTRICAL |
terminal | P_O2 | ELECTRICAL |
Description | This model describes an ideal splitter block which splits one input signal into two output signals without loosing any signal power. In real splitter blocks the signal would suffer loss due to mismatch.
Dependencies |
Logical Library | Design Unit/Design Entity
IEEE_proposed | ELECTRICAL_SYSTEMS
Source | See source code
Example | See test-bench