EMC for ICs > Models for EMC Simulation |

# Conclusion

This presentation is now completed. We detailed how an IC design methodology including EMC modeling and prediction may help saving money. We described the structure of the IC macro-model that enabled and accurate prediction of conducted/radiated emission, through a reduced set of simple elements. Then, we explained how the model can be feed with physical data at printed circuit, package, I/O and core level. We showed interesting correlation between measurements and simulation for a conducted 1ohm and TEM cell approaches, up to 1GHz. The future of EMC models, for bandwidth up to 18GHz and susceptibility have also briefly been discussed.

- EMC models can help earn/save money
- Macro-models of Ics include core modeling and package modeling
- The core model is based on current evaluation and on-chip capacitance
- The package model is based on RLC, and active I/V
- Good correlation has been achieved up to 1GHz
- Soon, requirements up to 3-10GHz