
FloresLoad.csv -- This file includes system load data from 2008 for the Island of Flores on a ten minute timestep. The first four columns are month, day, hour, and minute respectively, the 5th column is total system load, 6th is system load minus refrigerator load, and 7th is refrigerator load, all in kWh.

FloresHydro.csv – This file contains historical hydro dispatch data summed across all hydro plants in kWh. The time of each data point is listed in the corresponding row of FloresLoad.csv

FloresWindPower2008.csv – This file contains a synthetic time series of wind power output for E33 wind turbines on the island of Flores. This data was derived from wind speed data as described in Chapter 4. The power is normalized to maximum turbine output. The time of each data point is listed in the corresponding row of FloresLoad.csv   

FloresWindSpeed.csv – This file contains wind speed measurements taken at a height of 6.8m on Flores Island. Data is in m/s and the time of each data point is listed in the corresponding row of FloresLoad.csv

SMGLoad.csv – This file includes system load data from 2008 for the Island of Sao Miguel on a ten minute timestep. The first four columns are month, day, hour, and minute respectively, the 5th column is total system load, 6th is system load minus refrigerator load, and 7th is refrigerator load, all in kWh.

SMGBG.csv – This file contains historical biogas plant dispatch data from the year 2008 in kWh. The time of each data point is listed in the corresponding row of SMGLoad.csv.

SMGGT.csv -- This file contains historical Geothermal plant dispatch data from the year 2008 in kWh. This data represents the total output of all Geothermal plants. The time of each data point is listed in the corresponding row of SMGLoad.csv.

SMGHydro.csv -- This file contains historical hydropower plant dispatch data from the year 2008 in kWh. This data represents the total output of all hydropower plants. The time of each data point is listed in the corresponding row of SMGLoad.csv.

SMGWindPower2004.csv -- This file contains a synthetic time series of wind power output for E101 wind turbines on the island of Sao Miguel in the year 2004. This data was derived from wind speed data as described in Chapter 4. The power is normalized to maximum turbine output. The time of each data point is listed in the corresponding row of SMGLoad.csv   

SMGWindPower2007.csv -- This file contains a synthetic time series of wind power output for E101 wind turbines on the island of Sao Miguel in the year 2007. This data was derived from wind speed data as described in Chapter 4. The power is normalized to maximum turbine output. The time of each data point is listed in the corresponding row of SMGLoad.csv   

SMGWindPower2008csv -- This file contains a synthetic time series of wind power output for E101 wind turbines on the island of Sao Miguel in the year 2008. This data was derived from wind speed data as described in Chapter 4. The power is normalized to maximum turbine output. The time of each data point is listed in the corresponding row of SMGLoad.csv   

SMGWindSpeed2004.csv – This file contains wind speed measurements taken at a height of 6.0m on Sao Miguel Island in the year 2004. Data is in m/s and the time of each data point is listed in the corresponding row of SMGLoad.csv

SMGWindSpeed2007.csv – This file contains wind speed measurements taken at a height of 6.0m on Sao Miguel Island in the year 2007. Data is in m/s and the time of each data point is listed in the corresponding row of SMGLoad.csv


SMGWindSpeed2008.csv – This file contains wind speed measurements taken at a height of 6.0m on Sao Miguel Island in the year 2008. Data is in m/s and the time of each data point is listed in the corresponding row of SMGLoad.csv

Generator Configuration.xlsx and hydro_ramp.docx describe the generator cost, ramp rate, and capacity parameters.







